**VTH Function List 0515**

a) Add access control temperature monitoring device.

b) Real-time monitoring，event subscription, real-time report of events (including snapshot, temperature, time, user ID)

c) Abnormal events (temperature abnormalities) can be distinguished in the event list. Click the corresponding event to display it in a pop-up box.

d) Remote unlocking

e) VTH one-way talk (VTH to the access control terminal)